
Technical specification of the subject of the contract
Contract name: Anti-frost wind turbines with automatic control system Agis SK sro .

1. Anti-freeze wind turbines ... 3 pcs
The machine serves to protect trees from frost, the basic function is that the driven blade generates a flow of air (slightly warmer) from higher altitudes downwards and thus warmer air is achieved at the treetops than without the use of wind turbines. In this way, an increase in ground temperature by 4-5 C can be achieved. The machine consists of a tower, a rotor, an engine and a drive system between the engine and the rotor.
	[bookmark: _Hlk238476151]Manufacturer, type/brand of the offered goods:
	

	
Parameter description
	Minimum parameter requirements
	Your parameter (state meets / does not meet or state value)

	Tower material
	Galvanized steel
	

	Tower diameter/wall thickness
	Min. 500 mm / min. 0.8 mm
	

	Tower height
	Min. 10 m - max. 12 m
	

	Shovel - size
	Min. 5.5 m - max. 7 m
	

	Bucket material
	Fiberglass or carbon fiber
	

	Engine – aggregate
	Diesel generator
	

	HP performance
	Min. 140 HP – max. 180 HP
	

	Fuel tank
	At least 400 liters
	

	Protective mesh against pests and birds
	Required
	

	Drive system:
	Gearbox connected to cardan shaft
	

	Overload protection
	Required
	

	Rotor rotation around the axis 360
	Rotation around the axis in min. 4 – max. 7 minutes
	


	Territory protection (in ha)
	Min. 6 hectares
	

	[bookmark: _GoBack]Accessories: auxiliary heating via electric fan heater, quantity: 1 unit
	Electric heater,               min. 9 kW max. 15 kW
	


*Compliance with the requirement - the applicant shall indicate by selecting from the following options:
- the offer meets the specified technical parameter - the bidder states that it meets
- the offer does not meet the specified technical parameter - the bidder states it does not meet
- for each numerical parameter, the applicant shall indicate the exact parameter
Note, warning: the offer is accepted only if all parameters are met!
The price does not include the implementation of the foundation plate. The foundation plate is implemented by the customer based on the technical sheet of the wind turbine supplier.
Installation of the equipment on site as determined by the supplier in accordance with the project documentation on the affected plots: KN C 702/2, 703/1, 703/22, 704/1, 704/2, 706, 707/1, 707/2, 709, 712,713/2, 714, 715 in the cadastral area of Buzitka.
I also declare that the price offer includes delivery/transportation and installation of the subject of the contract and training of the operator at the contracting authority's location. 

2. Automatic control system - for anti-freeze wind turbines ... 3 pcs 
	Manufacturer, type/brand of the offered goods:
	

	
Parameter description
	Minimum parameter requirements
	Your parameter (state meets / does not meet or state value)

	automatic (automatic on and off according to the set temperature)
	Required
	

	Photovoltaic panel and accumulator
	Min. 15 W panel and / min. 105 Ah accumulator
	

	Weather monitoring
	Min. heat and wind sensor
	

	intelligent online connection and management
	Required
	



*Compliance with the requirement - the applicant shall indicate by selecting from the following options:
- the offer meets the specified technical parameter - the bidder states that it meets
- the offer does not meet the specified technical parameter - the bidder states it does not meet
- for each numerical parameter, the applicant shall indicate the exact parameter
Note, warning: the offer is accepted only if all parameters are met!
Installation of the equipment on site as determined by the supplier in accordance with the project documentation on the affected plots: KN C 702/2, 703/1, 703/22, 704/1, 704/2, 706, 707/1, 707/2, 709, 712,713/2, 714, 715 in the cadastral area of Buzitka.
I also declare that the price offer includes delivery/transportation and installation of the subject of the contract and training of the operator at the contracting authority's location.

	Name and surname
statutory representative:
	

	Signature and stamp:
	

	Place and date of signature:
	



