
Technical specification of the subject of the contract - assignment
Contract name: Walnut shaking and harvesting equipment  

1. Tree shaking device ... 1 pc.
	Manufacturer, type/brand of the offered goods:
	

	
Parameter description
	Minimum parameter requirements
	Your parameter (state meets / does not meet or state value)

	Mobile version
	Connection to the cardan shaft tractor
	

	Performance (number of trees/hour)
	Min. 100 trees / hour
	

	Tractor power requirements:
	Min 70 Horsepower max. 120 Horsepower
	

	Vibrating head
	Hydraulic adjustable, telescopic design
	

	Tree trunk diameter
(min. jaw opening for gripping the tree)
	at least 500 mm
	

	Head shift (from wheel to tree)
	Min. 2 m
	

	Height of shaking
	Min. From 0.5 m to min. 3 m
	

	Telescopic arm shift
	Min. 1 m
	

	Control
	Electronically, lever or joystick from the tractor cabin
	


*Compliance with the requirement - the applicant shall indicate by selecting from the following options:
- the offer meets the specified technical parameter - the bidder states that it meets
- the offer does not meet the specified technical parameter - the bidder states it does not meet
- for each numerical parameter, the applicant shall indicate the exact parameter
Note, warning: the offer is accepted only if all parameters are met!
I also declare that the price offer includes delivery/transport of the subject of the contract and training of the service personnel at the contracting authority's location. 

2. Automatic walnut harvesting equipment ... 2pcs
	Manufacturer, type/brand of the offered goods:
	

	
Parameter description
	Minimum parameter requirements
	Your parameter (state meets / does not meet or state value)

	Basic characteristics
	Automatic, self-propelled harvesting equipment nuts
	

	Engine power / fuel
	Min. 75 HP / diesel
	

	Drive
	4x4
	

	Shot width
	Min. 2 m
	

	Performance, collection capacity
	Min. 1 ha/hour.
	

	Sorting:
	Min. dirt separation
	

	Tank volume
	[bookmark: _GoBack]Min. 1.2 m3 - max. 5 m3
	

	Tray control
	Hydraulically
	

	Cabin with roof and air conditioning
	Required
	

	Harvesting other nuts
	Min. walnut, almond, hazelnut
	

	Automation, digitalization, robotization:

	Control
	Electronic control from the cab
	

	Monitoring
	At least 2 cameras
	

	Navigation
	Automatic guidance with accuracy up to +-3 cm. , GNSS +INS navigation systems, display, electric steering wheel
	

	Monitoring, logging, alerts
	Information about the engine, consumption, performance, distance traveled, error messages
	




*Compliance with the requirement - the applicant shall indicate by selecting from the following options:
- the offer meets the specified technical parameter - the bidder states that it meets
- the offer does not meet the specified technical parameter - the bidder states it does not meet
- for each numerical parameter, the applicant shall indicate the exact parameter
Note, warning: the offer is accepted only if all parameters are met!
I also declare that the price offer includes delivery/transport of the subject of the contract and training of the service personnel at the contracting authority's location.
	Name and surname
statutory representative:
	

	Signature and stamp:
	

	Place and date of signature:
	



