**Proposal for fulfilling the criteria**

**Pasta production machine**

|  |  |
| --- | --- |
| **Business name of the applicant:** |  |
| **Applicant ID number:** |  |
| **Applicant’s adress:** |  |
| **Legal representative:** |  |
| **Buyer:** | SIDAMA s.r.o. Jablonková 1122/34, 075 01 Trebišov |

## The pasta machine must form a single logical unit containing:

## Pasta machine with two independent vessels (one mixer, one extruder) including auger cooling.

## The order also includes complete technical documentation and operating instructions. The complete production technology must have safety devices in accordance with safety standards and meet all applicable legal standards in accordance with applicable legislation and international standards.

|  |  |
| --- | --- |
| **Main technical and functional requirements** | **Offered machine meets the requirement: YES / NO** |
| Mixer capacity - with a minimum tank capacity of 25 kg path |  |
| Production capacity in extrusion min. 90 kg / hour |  |
| Extruder with closed-loop cooling system, stainless steel screw with heat treatment and mixing of the mixture. |  |
| Rotary slicer with electrically adjustable speed for slicing pasta. |  |
| Bronze matrices with hard chrome and Teflon inserts (min. 10 types) for forming pasta with the possibility of producing various types of pasta such as: hairpins, threads, wide noodles, Slovak rice, targon, small, medium and large bottles, corrugated bottles, small and large mussels , elbows (macaroni), stars, propellers, crumbs with the addition of other types of matrices |  |
| all parts that are in contact with the product are made of stainless steel or material certified for the food industry |  |
| The design of the machine must be in accordance with the dimensions of the production room with a maximum clear height of 2.70 m and dimensions of 5.10 m x 5.50 m |  |

**Price offer**

|  |  |  |
| --- | --- | --- |
| Subject: | Name and type mark of the machine | Price (EUR, without VAT): |
| Pasta production machine |  |  |

Date: ----------------------------------------------------

Signature of the statutory representative