Technical specification of the subject of the contract - assignment
Contract name: Receiving hopper 
1. Receiving hopper ... 2pcs
	Manufacturer, type/brand of the offered goods:
	

	
Parameter description
	Minimum parameter requirements
	Your parameter (state meets / does not meet or state value)

	Mobile version
	Trailer on wheels
	

	Loading area capacity in m3
	Min. 15 m3 max. 24 m3
	

	Engine power in kW
	Max. 12 kW
	

	Adjustable material flow: minimum adjustable material flow t/h
	Min. From 0.5 to 15 t/ hour
	

	Width of the side outlet belt in mm.
	Min. 400 max. 600 mm
	

	Tray width in mm
 
	Min. 3000 max. 4000 mm
	

	Width of the main conveyor belt in mm
	From 1500 to 2500 mm
	

	Maximum machine height in mm
	Up to 3500 mm
	

	Automation, digitalization, robotization:
	Automatically operating device, without human intervention
	


*Compliance with the requirement - the applicant shall indicate by selecting from the following options:
- the offer meets the specified technical parameter - the bidder states that it meets
- the offer does not meet the specified technical parameter - the bidder states it does not meet
- for each numerical parameter, the applicant shall indicate the exact parameter
Note, warning: the offer is accepted only if all parameters are met!
I also declare that the price offer includes delivery/transport of the subject of the contract and training of the service personnel at the contracting authority's location.
	Name and surname
statutory representative:
	

	Signature and stamp:
	

	Place and date of signature:
	




