
Technical specification of the subject of the contract - assignment
Contract name: Shelling device ( cracker)    
1. Shelling device ( Cracker)   ... 2pcs
	Manufacturer, type/brand of the offered goods:
	

	
Parameter description
	Minimum parameter requirements
	Your parameter (state meets / does not meet or state value)

	Basic characteristics, functionality: walnuts are fed into the conical shelling machine via a hopper and conveyor belt; after shelling, most of the shells are removed by an air stream

	Performance, capacity of the nut sheller in the case of walnuts
	min 200kg/hour
	

	Crushing setting:
	adjustment of the crushing cone distance even during operation
	

	Engine power
	Min. 1.5 KW, max. 8 kW
	

	Vibrating hopper capacity
	0.75 m3 to 1.5 m3
	

	Belt conveyor, capacity min.
	capacity min. 500 kg/hour
	

	Separating shells from kernels
	With a fan, using flowing air
	

	Equipment suitable for shelling multiple nuts
	Min 3 types (walnuts and almonds, hazelnuts)
	

	Automation, digitalization, robotization:
	Automatically operating device without human intervention
	


*Compliance with the requirement - the applicant shall indicate by selecting from the following options:
- the offer meets the specified technical parameter - the bidder states that it meets
- the offer does not meet the specified technical parameter - the bidder states it does not meet
- for each numerical parameter, the applicant shall indicate the exact parameter
Note, warning: the offer is accepted only if all parameters are met!   
I also declare that the price offer includes delivery/transport of the subject of the contract and training of the service personnel at the contracting authority's location.
	Name and surname
statutory representative:
	

	Signature and stamp:
	

	Place and date of signature:
	



